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CONTROLS COMPANY ...

Temperature Controls Marketing Group
100 W. Victoria Street, Long Beach, CA 90805

NOTE: The following warning applies to installations using
L.P. Propane Gas. : oL .

Fig. 2. - WARNING :

To avoid .possible injury, fire and explosion, please read and follow
these precautions and all instructions on this appliance befare light-
ingthe pilot. This appliance uses L.P. (Propane) gas which is heavier
than air and wili remain atfloor level if there is aleak. Before lighting,

‘Operating ~lnstructions.for the
Robertshaw TS-11, J&K
Thermomagnetic Safety Valves.

sniff at floor level. It you smell gas, follow these directions.

1. Get all people out of the building. : c

2. PO NOT light matches. DO NOT turn glectric fights ar switches
on or off in area: DO NOT use an electric fan.to remove das |-
fromn area. o .

3. Shut off gas at L.P. tank outside of building. -

‘ . 4. Telephone gas company and fire department. Ask instructions.

Before hanging up, give your-name, addrass and phone number.
DO NOT go back into building. it help is coming wait for them to
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—
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TS-11K
(No Pilot Inlet)

arrive. |f your L.P. tank runs out of fusl, turn off gas at the appliance.
After L.P. tanik is refilied, appliance must be re-lit according to manu-
facturer’s instructions. ifthe gas control has besn exposed to WATER |
inany way, DONQT tryto use it. It must be replaced. DO NOT attempt-
repair on gas control or appliance.

Tampering is DANGEROUS and voids all warranties.

Installation Instructions

To avoid possible i'njury', fire and explosion, please read and
follow these precautions and all instructions on appliance.

Asthe manufaé;urer of this control, we recommend adjustments
be limited to the operations listed, which-our experience shows.
) are practical service operations. T '
I Installation’ or servicing of ‘gas‘appliances or controls must be.
: -performed by qualified service technicians. s .

1. - Follow shutdown and lighting instryctions on appliance.

. ,._.A.,,.___iw;,._.2'.'_..Shut=oﬁ-gas‘ahea,d@fécon}roLa\-line.~ya\ﬁg—qﬁ~1;£ﬂank:bei_ore-—~——

instaliation or servicing.. . .

3. Toinstall orremove control, use wrenchon maingasinlet and
outlet fittings only. ' T

4. Insert only correct size pipe or tubing into inlet or outlet of:

- control. Insertion. of any other object can cause internal

damage. .

5. Useonly new, unused controls as replacements. Do not reuse
old controls. .

6. When changing from naturaito L.P. or L.P. to natural-gas the
_ burner orifice and pilot aritice must also be changed. -

7 A sediment trap must be in- Fig-3
stalled in the gas supply line -
to the control. All piping must
comply with local codes and -1
ordinances and with the Nat- . ‘a«Min.
jonal Fuel Gas Code (ANSI:
Z223.1/NFPA, No. 54).

8. Make sure gas piping has been pressure tested before control
is connected. High pressure can damage the control, causing
a hazardous condition. Do not subject control to more than 1/2
PSI (14" W.C)) inlet pressure.

9. Make sure piping is clean and free from scale and burrs. Apply
asmall amount of pipe thread compound tothe gas inlet pipe
and connect pipe to the inlet of the control. Do not overtighten.

Do not use Teflon tape or Teflon pipe compound on gas inlet
connection. Thread compound should be used sparingly and
on male threads only, leaving first two threads clean. Pipe dope
or thread compound should never be used on female threads.
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IF YOU SMELL GAS: (A) Turn oft gas atline valve or meter.
(B) Open doors and windows. (C) Don't touch electrical
switches. (D) Extinguish any open flame. (E) Immediately

call your gas supplier from ‘outside” of building. Read
warning, Fig. 2. ' : .

Do not use pipe compound on autiet pipe or pilot connections.
10. The thermocouple nut should be started and turned all the
way in by hand. An additiona! quarter turn with a wrench will
then be sufficient to seat the lockwasher. CAUTION: Over-
tightening may damage thermocouple or magnet.
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