IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2018-05-22T12:28:06"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Default UI"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "i.terzi@specifiglobal.com" of Organization (no name given)
  Owner history of Person "i.terzi@specifiglobal.com" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "HT7" | object type "HT7" | names: "QF_Lincat_HT7:HT7:1020037" | material: materials ("QF_Metal-Stainless-Satin", "QF_Plastic-Red-Glossy", "QF_Plastic-Black-Matte", "QF_Plastic-Green-Glossy") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Electrical, Electrical - Loads

Types
  IFCBUILDINGELEMENTPROXYTYPE "HT7" | 1 occurrence | material: materials ("QF_Metal-Stainless-Satin", "QF_Plastic-Red-Glossy", "QF_Plastic-Black-Matte", "QF_Plastic-Green-Glossy") | property sets: Electrical, Graphics, Identity Data, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Specialty Equipment" (IFCLABEL)
    Family = "QF_Lincat_HT7: HT7" (IFCLABEL)
    Family and Type = "QF_Lincat_HT7: HT7" (IFCLABEL)
    Type = "QF_Lincat_HT7: HT7" (IFCLABEL)
    Type Id = "QF_Lincat_HT7: HT7" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Specialty Equipment" (IFCLABEL)
    Family Name = "QF_Lincat_HT7" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Foodservice Equipment Identifier = TRUE (IFCBOOLEAN)
    Furnished By = "" (IFCTEXT)
    Identify Quantity as Lot = FALSE (IFCBOOLEAN)
    Installed By = "" (IFCTEXT)
    Item Number = "" (IFCTEXT)
    Revision Code = "" (IFCTEXT)
    Specification by User = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "E1090320" (IFCTEXT)
    Assembly Description = "Food Service - Appliances & Equipment" (IFCTEXT)
    CSI MasterFormat = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "SILVERLINK 600 ELECTRIC COUNTER TOP FOUR PLATE BOILING TOP, 750MM WIDE" (IFCTEXT)
    Manufacturer = "LINCAT" (IFCTEXT)
    Masterspec = "" (IFCTEXT)
    Model = "HT7" (IFCTEXT)
    NAFEM Spec ID Number = "" (IFCTEXT)
    OmniClass Number = "23.40.40.14" (IFCTEXT)
    OmniClass Title = "Food Service Equipment" (IFCTEXT)
    SMACNA No = "" (IFCTEXT)
    Seismic Rating = "" (IFCTEXT)
    Serial Number = "" (IFCTEXT)
    Specification by Manufacturer = "" (IFCTEXT)
    Type Name = "HT7" (IFCTEXT)
    URL = "www.lincat.co.uk" (IFCTEXT)
    URL Cutsheet = "www.lincat.co.uk" (IFCTEXT)
    Weight in Pounds = 41.88778 (IFCREAL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Show Clearance = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 type object
    Show Logo = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "HT7" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "LINCAT" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1.87857327091023 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.11285451685902 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Conn Conduit = FALSE (IFCBOOLEAN)
    Elec Conn Connection Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Elec Conn RI Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Electric Connection Type = "" (IFCTEXT)
    Electrical Remarks = "" (IFCTEXT)
    Number of Poles = 1 (IFCINTEGER)
  Electrical | properties | on 1 type object
    Apparent Power = 7000. (IFCPOWERMEASURE) [WATT]
    Conn Plug = "" (IFCTEXT)
    Cycle = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    FL Amps = 30.5 (IFCELECTRICCURRENTMEASURE) [AMPERE]
    HP = "9.387140000000" (IFCTEXT)
    Max Overcurrent Protection = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Min Ckt Ampacity = 0. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Phase = 1 (IFCINTEGER)
    Volts = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Watts = 7000. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Status = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)